**TECH NOTES** *(revised 9/29/2022)*

**PEDESTRIAN RELATED**

TECH-1P COUNTDOWN ONLY DURING FLASHING PEDESTRIAN CHANGE INTERVAL.

TECH-2P PERCUSSIVE TONE ONLY DURING PEDESTRIAN WALK INTERVAL.

TECH-3P CONCURRENT PED PHASE ONLY COMES IN WHEN ACTUATED BY ASSOCIATED PUSH BUTTON

TECH-4P SPEECH MESSAGE “*(INSERT STREET NAME)*. WALK SIGN IS ON TO CROSS *(INSERT STREET NAME)*”. DURING PEDESTRIAN WALK INTERVAL. *(used where speech message is needed on both sides of the associated crosswalk)*

TECH-5P PERCUSSIVE TONE ONLY DURING PEDESTRIAN WALK INTERVAL FOR P# BUTTON(S). SPEECH MESSAGE “(*INSERT STREET NAME*). WALK SIGN IS ON TO CROSS (*INSERT STREET NAME)* DURING PEDESTRIAN WALK INTERVAL FOR P#A BUTTON(S). *(used where percussive tone is possible on one side of crosswalk and speech message is needed on the other side of the crosswalk)*

**COORDINATION/SYSTEM RELATED**

TECH-1S ARTERY DETECTORS TO BE NON-ACTUATING DURING COORDINATION.

TECH-2S TIMINGS SHOWN REFLECT FREE OPERATION.

TECH-3S ACTUAL COORDINATION INFORMATION TO BE DETERMINED BY THE COORDINATION SYSTEM.

TECH-4S SIGNAL MAY DOUBLE CYCLE IF PEDESTRIAN PHASE IS CALLED.

TECH-5S UNUSED TIME TO BE REALLOCATED.