Local Education Agency	State Project No.	Phase
School	Architect	Date

DAS - OFFICE OF SCHOOL CONSTRUCTION GRANTS & REVIEW (OSCG&R) PLAN REVIEW CHECKLIST

STAND-ALONE

WINDOW REPLACEMENT PROJECT

FORM SCG-3020

Do not use Not Applicable (N/A). Use “None”, “NPS” (Not in Project Scope), or explain condition.

Submit completed Pre-Bid Conformance Review (PCR) Checklist with this completed form.

Status column (by SCG staff): Accepted Open Item

Status
Drawings	Specifications
01.	Demo / Asbestos Abatement also complete FORM SCG-3011: (Asbestos/Hazardous Materials Abatement Checklist)
02.	Demo / PCB Abatement also complete FORM SCG-3012: (PCB Abatement and Management Checklist)
03.	Floor plans - for all floors (with all spaces identified)
04.	Rescue and ventilation (RV) windows identified on plans, elevations, and schedules (for all spaces occupied by students not served by a fully automatic fire suppression system)
05.	Dimension from floor to bottom of window opening for all rescue and ventilation (RV) windows (not dimension to top of sill)
06.	Clear opening dimensions for all rescue and ventilation (RV) windows
07.	Latching mechanism operation must be operable without the use of tools and, for new Educational Occupancies, height not more than 48” A.F.F.
08.	Security screens and bars must be easily openable without use of tools
09.	Egress doors and hardware (if part of project or in lieu of RV windows)